X-keys SPLAT Converter v1.0.1.3
October 19, 2004

This software is used to convert P.I. Engineering X-keys USB devices, which support SPLAT mode (SE X-keys), into SPLAT devices, or convert a SPLAT device into a Memory Resident Mode X-Keys USB device.  You must have the USB X-keys driver installed for SPLAT Converter to function properly.  If you do not have the driver installed you may download it at www.xkeys.com. Follow these directions to install this software.

1. Download the USBSplatConverterSetup.exe from P.I. Engineering website and save it to a local folder.
2. Unplug any X-keys USB devices from your system.
3. Double click on the USBSplatConverterSetup.exe.
4. Follow the Installation Wizard directions to install the software.
5. Plug the X-keys back into the USB port. 
6. Switch the X-keys into programming mode, (switch up, red dot visible on standard X-keys).
7. Run the software to SPLAT/UnSPLAT a X-keys USB device. 
Note: Click on "Get Mode" first when you want to either SPLAT or UnSPLAT a device.

Feel free to contact our technical department if you have further questions: tech@xkeys.com, 1-800-628-3185 or 517-655-5523.

To uninstall:
Follow the directions for installation and select "Completely Remove USB Splat Converter" when prompted or use the "Add/Remove Programs" option in Windows Control Panel.

P.I. Engineering, Inc.
101 Innovation Parkway
Williamston, MI 48895
1-800-628-3185 or 517-655-5523
http://www.xkeys.com

