
HIDBootloader

Plug in the trackball to be programmed while holding the center button.  
The tri color LED inside should blink red.

Start HIDBootloader.exe.
From the file menu sellect the desired hex file and load it. LEDOFF.HEX deactivates the internal LEDs except the DPI indicator. LEDON.HEX returns these LEDS to their original function.

Select the program item and program the unit.

Unplug and replug the trackball normally

